;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;
;       Texas Instruments Inc. Computer Segment PCIxx21 Configuration File
;
;
;This section is reserved for TI comments:
;
;
;NOTE: This file must be modified before running setup.exe from the root directory.
;
;
;INSTRUCTIONS:  By modifying this file, the Flashmedia driver registry parameters can be configured.
;
;               SMENABLE=1 (Default, Smartmedia enabled)
;               SMENABLE=0 (Smartmedia disabled)
;
;               The SDHost options can be configured as well.
;
;               SDSWITCH=0 (Default, SDIO-Microsoft Driver, SD-TI Driver, MMC-TI Driver)                
;               SDSWITCH=1 (SDIO-Microsoft Driver, SD-Microsoft Driver, MMC-TI Driver)
;               SDSWITCH=2 (SDIO-Microsoft Driver, SD-TI Driver, MMC-Microsoft Driver)
;               SDSWITCH=3 (SDIO-Microsoft Driver, SD-Microsoft Driver, MMC-Microsoft Driver)
;
;               Note that when SDSWITCH equals 2 or 3 MMC will not be operational since it is
;               not supported by Microsoft's driver.
;
;               Memory Stick PRO parallel mode can be disabled also (on dedicated socket only)
;
;               MSPARDEN=1 (Default)
;               MSPARDEN=0 (Disabled)
;
;               Debug Messages can be enabled
;
;               DBGMSGEN=0 (Disabled by Default)
;               DBGMSGEN=1 (Enabled for Debugging)
;
;               Smartmedia CIS check can be disabled (This is against the Smartmedia Specification!!)
;
;               SMCISCHK=1 (Enabled by Default)
;               SMCISCHK=0 (Disabled for Debugging purposes)
;       
;
;
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;; 



:1SMENABLE=0
:2SDSWITCH=1
:3MSPARDEN=1
:4DBGMSGEN=0
:5SMCISCHK=1



;END OF TICONFIG.TXT FILE


